**CLEMENTON FIRE MARSHAL’S OFFICE**

***STANDPIPE SYTEM/HOSE CABINET***

***TEST REPORT***

***Only this document will be accepted by the Borough of Clementon Bureau of Fire Safety for annual testing purposes as required by the New Jersey Uniform Fire Safety Code and applicable N.F.P.A. standards.***

**NOTE: USE THE TAB BUTTON TO MOVE THE CURSOR**

PROPERTY NAME:       DATE OF INSPECTION:   /  /20

PROPERTY ADDRESS:       INSPECTOR:

TESTING AGENCY NAME:

NJ-DFS BUSINESS PERMIT #      PHONE NUMBER:

*\*\*ALL STANDPIPE SYSTEMS SHALL MEETE THE FLOW DEMANDS REQUIRED AT THE TIME OF INSTALLATION*

1. TYPE OF SYSTEM:  WET  DRY CLASS I  CLASS II  CLASS III
2. FIRE DEPARTMENT CONNECTION PROPERLY IDENTIFIED:  YES  NO

LOCATION:

1. ARE VALVES IDENTIFIED WITH SIGN?  YES  NO
2. ALL STANDPIPE VALVES OPERATED AT ALL LOCATIONS:  YES  NO
3. ALL HOSE STATION VALVES OPERATED AT ALL LOCATIONS:  YES  NO
4. ANY MISSING STANDPIPE VALVE WHEELS?  YES  NO WERE MISSING WHEELS REPLACED?  YES  NO
5. ALL HOSE CABINET DOORS HAVE VISUAL IDENTIFICATION GLASS PANELS?  YES  NO
6. HOSE CABINET DOORS WITH NO GLASS PANELS HAVE APPROVED SIGN?  YES  NO
7. STANDPIPE THREADS COMPTIBLE WITH FIRE DEPT (N.S.T.)?  YES  NO

THREADS FREE OF DAMAGE?  YES  NO CONNECTIONS ACCESSIBLE?  YES  NO

1. MAIN DRAIN TEST?  YES  NO  N/A STATIC PRESSURE       PSI RESIDUAL PRESSURE       PSI
2. HYDROSTATIC TEST PERFORMED?  YES  NO DATE OF LAST HYDROSTATIC TEST:   /  /20
3. 5-YEAR FLOW TEST PERFORMED?  YES  NO IF YES, RECORD RESULTS BELOW:

OUTLET USED:       OUTLET SIZE:  1½  2½

STATIC PRESSURE       PSI RESIDUAL PRESSURE       PSI FLOW       GPM

FLOW & PRESSURE ACCEPTABLE:  YES  NO GAUGES RECALIBRATED?  YES  NO

DEFICIENCIES

SIGNATURE OF INSPECTION DATE:   /  /20

SIGNATURE OF OWNERS/REPRESENTATIVE DATE:   /  /20

Borough of Clementon

Bureau of Fire Safety

101 Gibbsboro Road

Clementon, NJ 08021

P: 856-783-0284, Ext. 123

F: 856-783-3419